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DORLAND System Control Technology Co., Ltd. recently launched Intrinsically Safe Explosion-proof Digital Card Camera EX Card Camera 02 Max, which uses front and rear dual camera lenses (64 million pixels) for easy selfies, supports EIS electronic image stabilization, supports autofocus, and presents clear near and far scenes. 
In addition, it is also suitable for outdoor construction, pipeline inspection, etc. It can be used in conjunction with various applications such as OA office systems, inspection positioning systems, data collection systems, etc. Especially suitable for harsh environments with hazardous explosions, such as petroleum, chemical, pharmaceutical, oil depots, tank farms, and other hazardous areas with flammable and explosive gases, facilitating timely communication between users, production, and scheduling.
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**8X optical variable lens
**Video resolution (5K/25FPS)
**Front and rear dual camera lenses
 (64 million pixels)
**720 * 1280 IPS high-definition Capacitive
 touch screen, supporting dual finger zoom
**EIS Electronic Anti Shake
**Manual zoom and focus of lens ring
**Custom Area Focusing
**Night vision full-color
**Auto focus
**WiFi wireless connection

	Certificate parameters

	Ex-Marking
	Ex ib IIC T4 Gb/ Ex ib IIIC T130℃ Db

	Certificate No.
	CLEx25.7874

	IP Grade
	IP54

	Specification parameters

	Feature
	**8X optical variable lens
**Video resolution (5K/25FPS)
**Front and rear dual camera lenses (64 million pixels)
**720 * 1280 IPS high-definition capacitive touch screen, supporting dual finger zoom
**EIS Electronic Anti Shake
**Manual zoom and focus of lens ring
**Custom Area Focusing
**Night vision full-color
**Auto focus
**WiFi wireless connection

	image resolution
	64M; 48M;  36M; 24M;  20M; 16M;  12M; 8M

	Video resolution
	5K25fps; 4K/30fps; 2.7K/30fps; 1080P/60fps; 1080P/30fps; 720P/60fps

	Front image sensor
	pixel
	8 million pixel CMOS sensor (up to 64MP interpolation)

	
	size
	1/2.8 inch

	Rear image sensor
	pixel
	13 million pixel CMOS sensor (up to 64MP interpolation)

	
	size
	1/3.06 inch

	Front lens parameters
	Lens Type
	9G4P

	
	perspective
	H (horizontal): 56.59 ° (W)~7.03 ° (T)
V (vertical): 32.09 ° (W)~4.00 ° (T)
D (diagonal): 64.51 ° (W)~8.03 ° (T)

	
	parameter
	Ff(F/1.8-2.6,  f=5.76-46.09mm)

	
	focusing distance
	0.2m(W)-0.4m(T)

	Rear camera parameters
	Lens Type
	7P

	
	perspective
	73.8° [(D73.8,H62,V48.5)°]

	
	parameter
	Ff(F/2.2,  f=3.37mm)

	
	focusing distance
	0.5m-0.8m

	Display screen
	panel type 
	IPS High Definition

	
	Display screen size
	3.6 inches

	
	Display screen resolution
	720*1280

	Touch screen
	Capacitive touch screen
	support

	Battery
	battery capacity
	3.7V 1500mAh

	
	endurance
	Video recording for 48 minutes

	Main functions
	Auto focus function
	support

	
	PC auxiliary functions
	webcam

	Supplementary lighting method
	Local fill light type
	LED flash

	
	External extended flash
	support

	Auxiliary focus light
	LED lights
	Close/Automatic

	file format
	photo
	JPG

	
	video
	MP4

	memory card
	Cache itself
	8Gb DDR4

	
	Local capacity
	Flash memory: N/A

	
	Maximum expansion capacity
	External storage: Single card slot: TF card slot (maximum 256GB)

	interface
	USB
	Type-C USB

	
	HDMI
	support

	
	MIC
	Support (3.5mm interface)

	
	memory card
	TF card slot (maximum 256GB)

	
	Tripod mounting hole
	1/4 inch standard screw hole

	Operation Menu
	functional mode
	Normal photography, portrait mode, landscape mode, creative filters, normal recording, slow motion recording, time-lapse recording, night mode

	
	Timed photo
	Off/3-second timer/5-second timer/10 second timer

	
	Continuous shooting
	3 sheets/5 sheets/10 sheets

	
	Exposure compensation
	Manual: ± 2.0EV

	
	focusing
	8X optical zoom

	
	Focusing method
	Manual Focus/Single Focus/Auto Focus

	
	sharpness
	Strong/Standard/Gentle

	
	Auto Shutdown
	Off/5 minutes/15 minutes/30 minutes

	
	ISO
	Automatic/100/200/400/800/1600/3200/6400

	
	shutter time 
	Automatic, 1/30, 1/60, 1/120, 1/240, 1/480

	
	Date setting
	Adjustable date stamp

	
	image quality
	Low/Medium/High

	
	white balance
	Automatic/Sunlight/Cloudy/Incandescent/Fluorescent

	
	light metering
	Center metering/Average metering/Spot metering

	
	fill light
	Off/Always On

	Computer recommendation system configuration
	PC system
	Win7/Win8/Win 10/win11

	
	USB
	Standard USB 2.0 port or higher

	shutter speed
	1/25Sec-1/480Sec

	language
	multiple languages

	Unit Weight
	415g (including battery), 390g (excluding battery)

	Product dimensions
	126.1*83.9*73.2mm
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Shenyang Product Quality Supervision And Inspection Institute
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( National quality inspection and testing center for low voltage explosion—proof electrical apparatus ( Liaoning) )
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#) & = Beijing Dorland System Control Technology Co., Ltd.
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Address:11-A1, 10th Floor, Building 2,Yard 1,Wangzhuang Road, Haidian
District, Beijing
R 8 R ARSI

Name of Product Intrinsically safe explosion-proof digital camera

25 B ® X Card Canera02  DC3.7V
ype Specification

B JB B E g ib IIC T4 Gb; Ex ib IIC T130°C Db
x-Marking

V- =
Product Standards Q/DLM 013-2023

a4 =
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The drawings, technical documents and the samples are verified and
certified according to standard(s) for safety as below:
GB/T3836.1-2021  MRXEVERREE 251 ¥4 B BAER
Explosive atmospheres-Part 1:Equipment-General requirements
GB/T3836.4-2021  MEKEMERREE 24 89 MARZEE “i” R HRE
Explosive atmospheres-Part 4:Equipment protection by intrinsic safety “i”
W OB T/ IR 1.5MERiP %S Enclosure Protection Rating: 1P54;
2.7 K 1 95 Ex battery 082 3.7V 1500mAh # d it fftes, HA (R #8% The product is

Explanation
powered by one Ex battery082 3.7V 1500mAh lithium battery with a protection circuit;
3. EHETE fE s B e AT 7o . EESRAIARED Charging, replacing, or removing the
battery in hazardous areas is strictly prohibited:
AR S T EAKTF 2W;  RF transmission power shall not exceed 2W;
SAEM R IR AL AR, SR ER B8 4o 4 2 R TH B A 25 When used in dusty
environments, measures should be taken to avoid dust accumulation on the enclosure
surface.
Erkk
>
it #
Approved by
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Date of issue oS ical 3 (Liaops®
YW E 2030-08-31
Valid date

ATE AU A SRR T P S 2, B RA AR SR RER S A SR ELE .
This certificate is only valid for the products which identify with the sample(s) tested and
verify certificate have the responsibility to ensure the products complying with relevant standard(s).
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